# LPOS Function

#### Purpose:

To return the current position of the line printer print head within the line printer buffer.

#### Syntax:

    LPOS(x)

#### Comments:

LPOS does not necessarily give the physical position of the print head.

x is a dummy argument.

If the printer has less than the 132 characters-per-line capability, it may issue internal line feeds and not inform the computer internal line printer buffer. If this has happened, the value returned by LPOS(x) may be incorrect. LPOS(x) simply counts the number of printable characters since the last line feed was issued.

#### Examples:

The following line causes a carriage return after the 60th character is printed on a line:

    100 IF LPOS(X)>60 THEN LPRINT CHR$(13)